{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Blad1"],"not_rendered":{"charts":0,"images":2,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Blad1","index":0,"n_rows":25,"n_cols":11,"rows_kept":25,"cut":false,"hidden":false,"merged":[]}
["Rookgassstroom",195000,"kg/uur",null,null,"Gasdruk",996,"millibara"]
[]
["Componenten ","M massa","Molfractie","Restant","Molfractie","Mol Massa","M Massa","Massa perc","Massa Perc","Gasstroom","Gasstroom"]
["Gas",null,"Nat (Volume)","Droog","Droog","Droog","Nat","W% nat","w% Droog","Nat","Droog "]
[null,null,"x 100 = vol%",null,null,"kg","kg",null,null,"kg/uur","kg/uur"]
["CO2",44,7.7200000000000005E-2,{"$f":"C6","v":7.7200000000000005E-2},{"$f":"D6/$D$16","v":9.5484636664198208E-2},{"$f":"E6*B6","v":4.2013240132247214},{"$f":"C6*B6","v":3.3968000000000003},{"$f":"C6*B6/$G$16","v":0.12413498239767561},{"$f":"E6*B6/$F$16","v":0.14203660999643994},{"$f":"H6*$B$1","v":24206.321567546744},{"$f":"J6","v":24206.321567546744}]
["CO",28,2.9999999999999997E-4,{"$f":"C7","v":2.9999999999999997E-4},3.7105428755517434E-4,{"$f":"E7*B7","v":1.0389520051544882E-2},{"$f":"C7*B7","v":8.3999999999999995E-3},{"$f":"C7*B7/$G$16","v":3.069753450719721E-4},{"$f":"E7*B7/$F$16","v":3.5124456075426736E-4},{"$f":"H7*$B$1","v":59.860192289034558},{"$f":"J7","v":59.860192289034558}]
["H2",2,8.0000000000000002E-3,{"$f":"C8","v":8.0000000000000002E-3},9.8947810014713162E-3,1.9789562002942632E-2,1.6E-2,5.8471494299423268E-4,6.6903725857955689E-4,114.01941388387537,{"$f":"J8","v":114.01941388387537}]
["N2",28,0.66149999999999998,{"$f":"C9","v":0.66149999999999998},0.81817470405915949,22.908891713656466,18.521999999999998,0.67688063588369851,0.77449425646315961,131991.72399732121,131991.72399732121]
["O2",32,6.1400000000000003E-2,{"$f":"C10","v":6.1400000000000003E-2},7.5942444186292354E-2,2.4301582139613553,1.9648000000000001,7.1802994999691769E-2,8.2157775353569593E-2,14001.584024939895,14001.584024939895]
["H2O",18,0.19159999999999999,0,0,0,3.4487999999999999,0.12603530596240684,0,24576.884662669334,0]
["SO2",64,1E-4,{"$f":"C12","v":1E-4},1.2368476251839146E-4,7.9158248011770536E-3,6.4000000000000003E-3,2.3388597719769307E-4,2.6761490343182279E-4,45.607765553550152,{"$f":"J12","v":45.607765553550152}]
["SO3",80,6.9999999999999999E-6,{"$f":"C13","v":6.9999999999999999E-6},8.6579333762874013E-6,6.9263467010299211E-4,5.5999999999999995E-4,2.0465023004798141E-5,2.3416304050284489E-5,3.9906794859356376,{"$f":"J13","v":3.9906794859356376}]
["HCl",36,2.9999999999999997E-8,{"$f":"C14","v":2.9999999999999997E-8},3.7105428755517434E-8,1.3357954351986276E-6,1.0799999999999998E-6,3.9468258652110697E-8,4.5160014954120087E-8,7.6963104371615861E-3,{"$f":"J14","v":7.6963104371615861E-3}]
[]
[null,null,{"$f":"SUM(C6:C15)","v":1.0001070300000001},0.80850703000000002,0.99999999999999989,29.579162818163745,27.363761079999996,1,1.0000000000000002,195000,170423.11533733067]
["Dichtheid rookgas in kg/Nm3",null,null,null,null,{"$f":"F16/22.4","v":1.3204983400965959},{"$f":"G16/22.4","v":1.2215964767857141}]
["Absolute vochtigheid rookgas",null,null,null,null,"x          =",{"$f":"J11/K16","v":0.14421098108682351},"kg/kg droog gas","Abs vochtigheid"]
[]
[null,null,null,null,null,"Quench",65,"oC Gewenst"]
[null,null,null,null,null,"RV",95,"%"]
[null,null,null,null,null,"pw max",{"$f":"psat_t(G20)*1000","v":250.41097904236148},"milli bara"]
[null,null,null,null,null,"pw",{"$f":"G22*G21/100","v":237.8904300902434},"milli bara"]
[null,null,null,null,null,"x max",{"$f":"B11/F16*G23/(G1-G23)","v":0.1909552573045242},"kg/kg droog rookgas"]
[null,null,null,null,null,"Verdamping",{"$f":"(G24-G18)*K16","v":7966.3051772092485},"kg water/ uur"]