{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Blad1"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Blad1","index":0,"n_rows":36,"n_cols":16,"rows_kept":36,"cut":false,"hidden":false,"merged":[[3,1,3,3],[9,1,9,3],[14,1,14,3],[20,1,20,3],[1,1,1,3]]}
[]
[null,"Turbine zonder aftap"]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"C5","v":80},"Bara"]
[null,"A"]
[null,"Stoomdruk",80,"Bara"]
[null,"Stoom temp",460,"oC",null,"h    kJ/kg",null,null,null,null,null,null,{"$f":"C6","v":460},"oC"]
[null,"Enthalpie",{"$f":"h_pt(C5,C6)","v":3298.9095862571976},"kJ/kg"]
[null,"Entropie",{"$f":"s_pT(C5,C6)","v":6.5929390933287007},"kJ/kg.K"]
[null,"Spec Volume",{"$f":"v_pT(C5,C6)","v":3.8928984050267471E-2},"m3/kg"]
[null,"B",null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"C11","v":0.05},"Bara"]
[null,"Condensor druk",0.05,"Bara"]
[null,"Dampgehalte",{"$f":"x_ps(C11,C8)","v":0.77253692399941798}]
[null,"Enthalpie",{"$f":"h_px(C11,C12)","v":2009.6220744336217},"kJ/kg"]
[]
[null,"C"]
[null,"Inwendig Rendement",0.85]
[null,"Enthalpie",{"$f":"C7-(C7-C13)*C16","v":2203.015201207158},"kJ/kg"]
[null,"Dampgehalte",{"$f":"x_ph(C11,C17)","v":0.85235249475959329}]
[null,"Entropie",{"$f":"s_ph(C11,C17)","v":7.2248917075255905},"kJ/kg.K"]
[null,"Mechanisch Rendement",0.96]
[]
[null,"ms",22,"kg/s"]
[null,"Dh0",{"$f":"C7-C13","v":1289.2875118235759},"kJ/kg"]
[null,"Dhp",{"$f":"C7-C17","v":1095.8943850500395},"kJ/kg"]
[null,"Pth",{"$f":"C22*C23","v":28364.325260118669},"kW"]
[null,"Pinw",{"$f":"C22*C23*C16","v":24109.676471100869},"kW"]
[null,"Pe",{"$f":"C22*C23*C16*C20","v":23145.289412256832},"kW"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"C18","v":0.85235249475959329}]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"C12","v":0.77253692399941798}]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"s   kJ/kg.K"]